IFC building model
Schema: "IFC2X3"
Description: "IFC2X3"
File name: "AN-R.IFC"
Time stamp: "2021-09-27T13:12:20"
Preprocessor: "SwIFC"
Originating system: "SolidWorks 2021"
Application: "SolidWorks 2019" version "19.0" identifier "SolidWorks" by Organization "SolidWorks" id "SW" description "SolidWorks"

People and organizations
  Person (no name given) of Organization ""
  Owner history of Person (no name given) of Organization "" | application "SolidWorks 2019" version "19.0" identifier "SolidWorks" by Organization "SolidWorks" id "SW" description "SolidWorks" | change ADDED | created 1632748340 (2021-09-27T13:12:20Z) | last modified 1632748340 (2021-09-27T13:12:20Z) by Person (no name given) of Organization "" with "SolidWorks 2019" version "19.0" identifier "SolidWorks" by Organization "SolidWorks" id "SW" description "SolidWorks"

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE

Spatial structure
IFCPROJECT "Default Project"
  IFCSITE "Default Site" | latitude 0° 0′ 0″ | longitude 0° 0′ 0″ | elevation above sea level 0.000000000000000000
    IFCBUILDING "Default Building"
      IFCBUILDINGSTOREY "Default Storey" | elevation 0.000000000000000000
        contains 1 element
          1 x IFCELEMENTASSEMBLY | object type "AN-R" | names: "AN-R" | parts: 7 IFCBUILDINGELEMENTPROXY | property sets: SolidWorks Custom Properties, PSet_Mass_Property

Property sets
  SolidWorks Custom Properties | properties | on 4 objects (3 IFCBUILDINGELEMENTPROXY, 1 IFCELEMENTASSEMBLY)
  SolidWorks Custom Properties | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Gewicht = "62.58" (IFCLABEL)
    Material = "St12" (IFCLABEL)
  SolidWorks Custom Properties | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Gewicht = "40.41" (IFCLABEL)
    Material = "St12" (IFCLABEL)
    Oberfläche = "verzinkt" (IFCLABEL)
    Version 1 = "QA - quadr.Blende,Mh max 4,0m Fläche" (IFCLABEL)
    Version 2 = "QB - quadr.Blende,Mh max 4,0m Wege" (IFCLABEL)
    Version 3 = "QF - quadr.Blende,Mh max 8,0m Fläche" (IFCLABEL)
    Version 4 = "QW - quadr.Blende,Mh max 9,0m Wege" (IFCLABEL)
    Version 5 = "RA - runde Blende,Mh max4,0m Fläche" (IFCLABEL)
    Version 6 = "RB - runde Blende,Mh max4,0m Wege" (IFCLABEL)
    Version 7 = "RF - runde Blende,Mh max8,0m Fläche" (IFCLABEL)
    Version 8 = "RW - runde Blende,Mh max4,0m Wege" (IFCLABEL)
  SolidWorks Custom Properties | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Version 1 = "B - LED+Wege Linse Mh.3,5m 150Lm" (IFCLABEL)
    Version 2 = "C - sym/asym.Linse (SET) f.Mh3,5m" (IFCLABEL)
  SolidWorks Custom Properties | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Version 1 = "AX3- AT.DS & BS,LFP 1,6Ah 3h 140Lm" (IFCLABEL)
    Version 2 = "AX3DA - AT.DS&BS,LFP1,6Ah,3h 140Lm DLI" (IFCLABEL)
    Version 3 = "AX8 - AT.DS & BS,LFP 3,2Ah 8h 140Lm" (IFCLABEL)
    Version 4 = "AX8DA - AT.DS&BS,LFP 3,2Ah8h 140Lm DLI" (IFCLABEL)
    Version 5 = "C - zentr.Vers. AC/DC Adressmodul" (IFCLABEL)
    Version 6 = "E - für zentrale Versorgung AC/DC" (IFCLABEL)
    Version 7 = "FM3 - AT.DS&BS,LFP3,2V 3h 2/4W RC250" (IFCLABEL)
    Version 8 = "FM8 - AT.DS&BS,LFP3,2V 8h 2/4W RC250" (IFCLABEL)
  PSet_Mass_Property | properties | on 1 object (1 IFCELEMENTASSEMBLY)
    Area Measure = 0.1023782836033652194 (IFCAREAMEASURE) [SQUARE_METRE]
    Mass Measure = 0.2211370157951265125 (IFCMASSMEASURE)
    Volume Measure = 0.0001312256049493655085 (IFCVOLUMEMEASURE) [CUBIC_METRE]